{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Game","Feldata"],"not_rendered":{"charts":1,"images":11,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Game","index":0,"n_rows":18,"n_cols":8,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
["Převod",null,null,null,"PLYNOVÝ PEDÁL:"]
["Rychlost",null,"km/h",null,null,null,0,{"$f":"G10/100","v":0}]
["Otáčky",null,"RPM"]
["Zrychlení",null,"km/h/s"]
["Výkon",null,"kW"]
["Krouťák",null,"N·m",null,"ŘADÍCÍ PÁKA:"]
["Spotřeba",null,"l / 100km"]
["Uplynulý čas"]
["Ujetá vzdálenost",null,"km"]
["Průměrná rychlost",null,"km/h"]

{"sheet":"Feldata","index":1,"n_rows":36,"n_cols":11,"rows_kept":36,"cut":false,"hidden":false,"merged":[[0,6,0,8],[1,6,1,8]]}
[null,null,null,null,null,null,"modrý text = data vycucaná z prstu"]
[null,null,null,null,null,null,"šedé buňky = vzorce → NEMĚNIT!"]
[]
[]
[null,null,null,null,null,"PLYN:",100,{"$f":"G5/100","v":1},"Pozn.: tento plyn je jen pro graf a nepromítne se do hry"]
[]
[null,null,null,null,null,"VÝKONOVÉ CHARAKTERISTIKY"]
["RŮZNÉ"]
["hmotnost:",935,"kg","f [RPM]","T max [N·m]","T diss","T zdroj","T model","P [kW]"," Příkon [kW]","účinnost"]
["lineární odpor:",250,"N",500,55,16,{"$f":"E10+F10","v":71},{"$f":"G10*$H$5-F10","v":55},{"$f":"2*PI()*D10/60*E10/1000","v":2.8797932657906435},{"$f":"$B$36*$B$31*$D10/60/2","v":19.342986857014413},{"$f":"I10/J10","v":0.14888048506047216}]
["kvadratický odpor:",0.51,"N*s2/m2",1000,78,18,{"$f":"E11+F11","v":96},{"$f":"G11*$H$5-F11","v":78},{"$f":"2*PI()*D11/60*E11/1000","v":8.1681408993334621},38.685973714028826,{"$f":"I11/J11","v":0.21113959699485144}]
[null,null,null,1500,83,20,103,83,13.037609512397642,58.028960571043243,0.22467418654580346]
[null,null,null,2000,88,23,111,88,18.430676901060121,77.371947428057652,0.23820877609675548]
[null,null,null,2500,93,26,119,93,24.347343065320896,96.714934285072076,0.25174336564770744]
["PŘEVODOVKA",null,null,3000,97,30,127,97,30.473448739820991,116.05792114208649,0.26257103728846903]
["r [m]",0.28000000000000003,null,3500,102,35,137,102,37.384952577718536,135.40090799910089,0.27610562683942108]
["fix",4.1669999999999998,null,4000,105,40,145,105,43.982297150257104,154.7438948561153,0.28422638056999233]
[1,3.3079999999999998,null,4500,102,46,148,102,48.066367599923844,174.08688171312971,0.27610562683942114]
[2,1.913,null,5000,95,53,148,95,49.741883681838395,193.42986857014415,0.25715720146808829]
[3,1.2669999999999999,null,5500,81,61,142,81,46.652650905808422,212.77285542715856,0.2192603507254226]
[4,0.92700000000000005,null,6000,70,70,140,70,43.982297150257111,232.11584228417297,0.18948425371332822]
[5,0.71699999999999997,null,6500,57,80,137,57,38.798669271833944,251.45882914118738,0.15429432088085296]
["R",2.923,null,7000,41,92,133,41,30.05456971934235,270.80181599820179,0.1109836343178065]
[null,null,null,7500,23,106,129,23,18.06415775814131,290.1448028552162,6.225911193437926E-2]
["KONSTANTY",null,null,8000,0,120,120,0,0,309.48778971223061,0]
["λ",1.01]
["R [J/K/mol]",8.3140000000000001]
["p [kPa]",101.325,null,null,null,null,"Tdiss under 500 RPM"]
["V [l]",1.2889999999999999,null,null,null,null,15,"N*m"]
["T sání [K]",298,null,null,null,null,"Tdiss over 8000 RPM"]
["ΔHsp [kJ/g]",46.4,null,null,null,null,120,"N*m"]
["x O2",0.21]
["stechiometrie",12.5]
["M oktan [g/mol]",114.1]
["rho [g/l]",750]
["m fuel / cycle [g]",{"$f":"B28*B29/B27/B30*B32/B26/B33*B34","v":0.10004993201904008}]